







Deter: switch to configure as common cathode or anode

data\_in: 0-3 for bcd data

4-6 for address

7 for en on the falling edge.